Instruction Description

ASCII Protocol Command

The transmission of commands and return information is in ASCII format. All commands start with command characters and parameters (if any, in hexadecimal units) and stop with <CR> (0x0D hex), while return information will start with <LF> (0x0A hex), the first character of the command, and stop with <CR><LF>. If the command does not match the corresponding settings, the return information will be <LF>X<CR><LF>.

For example:

PC or Host: <LF>S<CR>

Reader return message: <LF>S01234567<CR><LF>